****

**Features:**

* Freestanding Tub
* Feet at the bottom of the tub
* Center drain
* 59” (1500mm) x 30” (750mm) x 23” (580mm)

**Material:**

* Acrylic with reinforced FRP

**Codes/ Standards:**

* CSA B45.5-11/IAPMO Z124

**Technical Information** (All product dimensions are nominal)

INSTALLED SIZE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_59 x 30 x23 in. (1500 x 750 x 580mm)

DRAIN LOCATION: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Center

WEIGHT\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_110.2Lb. (50Kg)

CAPACITY ：\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 522.5Lb. (237Kg)

GAL. TO OVERFLOW\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 52 Gal. （237L)

BATHING WELL AT SUMP\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 59X30 in. (1500x750mm)

BATHIING WELL AT RIM\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_40X17 in.(1020x440mm)

WATER DEPTH TO OVERFLOW\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ 14.2 In. (360mm)



Cut Sheet of the tub

DIMENSIONS OF FIXTURES ARE NOMINAL AND MAY VARY WITHIN THE RANGE OF TOLERANCES ESTABLISHED BY ANSI STANDARDS Z124.1.2-2005

**NOTES:**

* Refer to the installation instructions supplied with this product for additional information.
* Provide suitable reinforcement for all supports.

**IMPORTANT:** Dimensions of fixtures are nominal and may vary within the range of tolerances established by ANSI standard Z124.1

These measurements are subject to change. No responsibility is assumed for use of superseded or voided leaflet.